Test Coverage Report for Board: 80-MB0M80-A01
Shorts Test Coverage Summary
IC Component Vector(Digital) Test Coverage Summary
IC Component Vectorless(Testjet) Test Coverage Summary
Non-IC Component Vectorless(Testjet) Test Coverage Summary
IC Component Vectorless(CL_Diode) Test Coverage Summary
IC Component Socket Test Coverage Summary
No Test Component - IC Type
IC Component Pin Level Test Coverage Summary
Analog Component(MDA) Test Coverage Summary
No Test Component - Analog(MDA) Type
Tested Component Summary
Analog(MDA) Type Untestable Component
Analog(MDA) Drive Through Component
Shorts Test Coverage Summary |

Total Number of Nets = 2258 Total Number of Nets Testable = 1731 Total Percentage of Nets Testable(1731/2258) = 76.66% Total Number of Nets Tested = 1731 Total Percentage of Nets Tested (1731/1731) = 100.00%

ˇ¶TOP
IC Component Vector(Digital) Test Coverage Summary |
ˇ¶TOP
IC Component Vectorless(Testjet) Test Coverage Summary |
ˇ¶TOP
Non-IC Component Vectorless(Testjet) Test Coverage Summary |
ˇ¶TOP
IC Component Vectorless(CL_Diode) Test Coverage Summary |
PartsName | Loc | Side | TotalPin | Testable | Tested | CoverageRate | Comment
UL1U1 | B1 | T | 37 | 10 | 8 | 80.0 |
UF1U1 | B4 | T | 8 | 6 | 5 | 83.3 |
U31U6 | C1 | T | 14 | 12 | 8 | 66.7 |
U3CP1 | C1 | T | 8 | 2 | 2 | 100.0 |
UAU1 | A1 | T | 48 | 25 | 25 | 100.0 |
UGU1 | E1 | T | 38 | 8 | 3 | 37.5 |
UGU2 | E1 | T | 53 | 14 | 11 | 78.6 |
UK1U1 | B2 | T | 128 | 61 | 61 | 100.0 |
UOU1 | B1 | T | 64 | 48 | 42 | 87.5 |
UO310 | F4 | T | 18 | 2 | 2 | 100.0 |
UO320 | B1 | T | 18 | 2 | 2 | 100.0 |
UP101 | F3 | T | 57 | 43 | 43 | 100.0 |
UP102 | F2 | T | 11 | 3 | 3 | 100.0 |
UP103 | F2 | T | 11 | 3 | 3 | 100.0 |
UP104 | F2 | T | 11 | 3 | 3 | 100.0 |
UP201 | F3 | T | 11 | 3 | 3 | 100.0 |
UP202 | F2 | T | 11 | 3 | 3 | 100.0 |
UP501 | F4 | T | 13 | 8 | 8 | 100.0 |
UP503 | C4 | T | 13 | 3 | 3 | 100.0 |
UP704 | B4 | T | 16 | 4 | 4 | 100.0 |
UP705 | B4 | T | 8 | 5 | 3 | 60.0 |
UP706 | D2 | T | 13 | 7 | 7 | 100.0 |
USU1 | B3 | T | 837 | 242 | 242 | 100.0 |
ˇ¶TOP
IC Component Socket Test Coverage Summary |
ˇ¶TOP
No Test Component - IC Type |
Component | Comment
UBU3 |
U31P1 |
U31P3 |
U31U1 |
U31U5 |
U3CP2 |
U3U1 |
UDIA1 |
UDIA2 |
UDIB1 |
UDIB2 |
ULGA1 |
UO2U1 |
UPCI1 |
UPEX1 |
UPEX2 |
UPCX1 |
UP302 |
UP701 |
Total Number of IC Components Testable | = 43
Total Number of IC Components Tested | = 24
ˇ¶TOP
IC Component Pin Level Test Coverage Summary |
PartsName | Loc | Side | TotalPin | Testable | Tested | CoverageRate | Comment
UL1T1 | C1 | T | 24 | 12 | 9 | 75.0 |
UL1U1 | B1 | T | 37 | 15 | 8 | 53.3 |
UF1U1 | B4 | T | 8 | 6 | 5 | 83.3 |
U31U6 | C1 | T | 14 | 12 | 8 | 66.7 |
U3CP1 | C1 | T | 8 | 5 | 2 | 40.0 |
UAU1 | A1 | T | 48 | 37 | 25 | 67.6 |
UGU1 | E1 | T | 38 | 20 | 3 | 15.0 |
UGU2 | E1 | T | 53 | 16 | 11 | 68.8 |
UK1U1 | B2 | T | 128 | 80 | 61 | 76.2 |
UOU1 | B1 | T | 64 | 60 | 42 | 70.0 |
UO310 | F4 | T | 18 | 3 | 2 | 66.7 |
UO320 | B1 | T | 18 | 3 | 2 | 66.7 |
UP101 | F3 | T | 57 | 51 | 43 | 84.3 |
UP102 | F2 | T | 11 | 6 | 3 | 50.0 |
UP103 | F2 | T | 11 | 6 | 3 | 50.0 |
UP104 | F2 | T | 11 | 6 | 3 | 50.0 |
UP201 | F3 | T | 11 | 6 | 3 | 50.0 |
UP202 | F2 | T | 11 | 6 | 3 | 50.0 |
UP501 | F4 | T | 13 | 9 | 8 | 88.9 |
UP503 | C4 | T | 13 | 6 | 3 | 50.0 |
UP704 | B4 | T | 16 | 11 | 4 | 36.4 |
UP705 | B4 | T | 8 | 6 | 3 | 50.0 |
UP706 | D2 | T | 13 | 9 | 7 | 77.8 |
USU1 | B3 | T | 837 | 340 | 242 | 71.2 |
Total: |  |  |  | 731 | 503 | 68.8
ˇ¶TOP
Analog Component(MDA) Test Coverage Summary |
|  |  | | | (Untestable Components) | | |
CompType |  | Total | | |  | NoComp | NoNail | Parallel |  | | | Testable | Tested | NoTest | CoverageRate(%)
Jumper | : | 584 | - | ( | 412 | 25 | 0 | ) | = | 147 | 136 | 11 | 92.5
Resistor | : | 443 | - | ( | 0 | 1 | 9 | ) | = | 433 | 433 | 0 | 100.0
Capacitor | : | 970 | - | ( | 490 | 109 | 206 | ) | = | 165 | 162 | 3 | 98.2
Bead/Coil | : | 0
Diode | : | 62 | - | ( | 25 | 0 | 0 | ) | = | 37 | 37 | 0 | 100.0
Transistor | : | 158 | - | ( | 52 | 0 | 0 | ) | = | 106 | 106 | 0 | 100.0
FET | : | 0
Others | : | 0
Total | : | 2217 | - | ( | 979 | 135 | 215 | ) | = | 888 | 874 | 14 | 98.4
ˇ¶TOP
No Test Component - Analog(MDA) Type |
Component | TestType | Comment
CL1C10 | (C) | BP
JAUDIO | (J) |
JBATTERY | (J) |
JKBMSU78 | (J) |
JSATA6G1 | (J) |
JSATA6G2 | (J) |
JSATA6G3 | (J) |
JSATA6G4 | (J) |
JSATA6G5 | (J) |
JSATA6G6 | (J) |
CSC143 | (C) | BP
CSC144 | (C) | BP
JUSB35 | (J) | Parallel JKBMSU78_4_5
JVGA | (J) |
Total Number of MDA Components Testable | = 888
Total Number of MDA Components Tested | = 874
ˇ¶TOP
Tested Component Summary |

Total Number of Components Found in PARTS.ASC: 2260 Total Number of Components Testable = 931 Total Number of Components Tested = 898 Total Percentage of Components Tested = 96.46% Comment: ---------------------- 1. Total testable components = Analog(MDA) add IC testable components. 2. Total tested components = Analog(MDA) add IC tested components. 3. The analog(MDA) components will not be testable if the part is not mounted, no nail or parallel. 4. The component found in PARTS.ASC will not be testable if the pins are less than 2.

ˇ¶TOP
Analog(MDA) Type Untestable Component |
1. No Component |
Jumper: | RJR25, RJR27, RJR28, L1L24, RL1R81, RL1R88, RL1R94, RL1R95, RL1R96, RL1R97
| JL1TJ1, RD3R24, RD3R25, RD3R31, RD3R32, LU31L1, LU31L2, LU31L3, LU31L4, RU31PR1
| RU31PR11, RU31PR12, RU31PR2, RU31PR21, RU31PR22, RU31PR29, RU31PR3, RU31PR30
| RU31PR4, RU31PR9, RU31PU5R1, RU31PU5R2, RU31R1, RU31R10, RU31R11, RU31R12
| RU31R13, RU31R14, RU31R15, RU31R16, RU31R3, RU31R30, RU31R31, RU31R32, RU31R33
| RU31R34, RU31R35, RU31R6, RU31R7, RU31U5R11, RU31U5R5, RU31U5R6, RU31U5R7
| RU31U5R8, LU3CL1, LU3CL2, LU3CL3, LU3CL4, RU3CR15, RU3CR16, RU3CR17, RU3CR18
| RU3CR188, RU3CR189, RU3CR19, LU3EF1, LU3EF3, LU3EL1, LU3EL2, RU3ER13, RU3ER15
| RU3ER16, RU3ER19, RU3ER81, RU3ER82, RU3ER83, RU3ER84, RU3ER85, RU3ER86, RU3ER87
| RU3ER88, RU3PR1, LAL5, LAL6, RAR19, JCPUJP9, RGR204, RGR205, RGR206, RGR207
| RGR208, RGR209, RGR210, RGR211, RGR214, RGR216, RGR42, LGU1L4, LGU1L5, LGU1L6
| RGU1R18, RGU1R19, RGU1R40, RHR104, RHR127, RHR131, RHR156, RHR158, RHR191
| RHR201, RHR22, RHR91, RHR92, RHR93, RHR94, RHR95, RHR97, RHR98, RHR99, JK1JP2
| LK1L51, LK1L52, RK1PR10, RK1PR9, RK1R2, RKR5, RO1R101, RO1R102, RO1R103, RO1R105
| RO1R106, RO1R107, RO1R108, RO1R109, RO1R11, RO1R111, RO1R112, RO1R122, RO1R134
| RO1R140, RO1R142, RO1R145, RO1R146, RO1R147, RO1R171, RO1R190, RO1R191, RO1R192
| RO1R193, RO1R195, RO1R196, RO1R20, RO1R36, RO1R42, RO1R45, RO1R70, RO1R71
| RO1R72, RO1R8, RO1R99, ROR200, ROR203, ROR210, ROR211, ROR219, ROR251, ROR304
| ROR314, ROR324, ROR764, ROR765, ROU310R1, ROU320R1, JPJP101, JPJP102, JPJP103
| JPJP104, JPJP105, JPJP106, JPJP201, JPJP202, JPJP203, JPJP204, JPJP301, JPJP302
| JPJP303, JPJP505, JPJP506, JPJP704, JPJP707, JPJP708, JPJP709, RPR108, RPR110
| RPR142, RPR151, RPR152, RPR162, RPR182, RPR191, RPR196, RPR200, RPR203, RPR204
| RPR205, RPR216, RPR220, RPR221, RPR222, RPR227, RPR301, RPR302, RPR303, RPR306
| RPR308, RPR310, RPR317, RPR318, RPR319, RPR320, RPR321, RPR322, RPR324, RPR325
| RPR326, RPR327, RPR329, RPR330, RPR331, RPR430, RPR432, RPR433, RPR522, RPR527
| RPR557, RPR558, RPR562, RPR566, RPR571, RPR572, RPR575, RPR602, RPR703, RPR704
| RPR705, RPR706, RPR709, RPR714, RPR715, RPR716, RPR725, RPR736, RPR738, RPR745
| RPR748, RPR751, RPR770, RPR771, RPR772, RPR773, RPR774, RPR776, RPR777, RPR778
| RPR779, RPR780, RPR781, RPR782, RPR804, RPR807, RPR813, RSBPWR, LSLX1, LSLX2
| LSLX3, LSLX4, LSLX5, LSLX6, LSLX7, LSLX8, RSR1, RSR124, RSR126, RSR133, RSR146
| RSR15, RSR1612, RSR1613, RSR1614, RSR1615, RSR1616, RSR1618, RSR1619, RSR1620
| RSR1622, RSR1624, RSR1625, RSR1627, RSR1630, RSR1631, RSR1632, RSR1635, RSR1636
| RSR1638, RSR1641, RSR1644, RSR17, RSR175, RSR180, RSR181, RSR192, RSR193, RSR200
| RSR201, RSR23, RSR24, RSR243, RSR25, RSR26, RSR27, RSR28, RSR29, RSR30, RSR305
| RSR31, RSR32, RSR33, RSR35, RSR36, RSR37, RSR39, RSR41, RSR61, RSR618, RSR63
| RSR631, RSR64, RSR66, RSR68, RSR70, RSR71, RSR72, RSR78, RSR79, RSR8, RSR83
| RSR93, RSR94, RSR95, RSR96, RSR97, RSRP2, RSRP5, RSRP6, RSRP7, RSRP8, RSRP9
| LTL1, RTMR1, RTMR2, JTPM, RTR1, RTR10, RTR11, RTR13, RTR17, RTR18, RTR19, RTR20
| RTR21, RTR26, RTR29, RTR30, RTR32, RTR33, RTR38, RTR39, RTR40, RTR41, RTR44
| RTR48, RTR49, RTR6, RTR7, RTR74, RTR84, RTR85, RTR86, RTR87, RTR88, RTR89
| RTR91, RTR92, RTR93, RTR94, RTR95, RTR96, LULA33, LULA34, LULB33, LULB34, RUR731
| RUR735, RUR750, RUR751, RUR752, RUR753, RUR754, RUR756, RURN31, RURN32, JVRMW100
Capacitor: | CBC6, CEC2, CTC1, CTC15, CTC16, CTC17, CTC18, CTC19, CTC20, CTC4, CTC43
| CTC44, CTC5, CTC6, CTC8, CXC71, CXC73, CXC74, CL1C12, CL1C13, CL1C14, CL1C94
| CL1C95, CL1C96, CL1C97, CL1C98, CL1U1C211, CL1U1C32, CD3C1, CD3C14, CD3C19
| CD3C2, CD3C22, CD3C33, CD3C34, CD3C93, CD4C7, CD4C8, CPC111, CPC113, CPC120
| CPC130, CPC131, CPC135, CPC136, CPC149, CPC150, CPC151, CPC159, CPC162
| CPC163, CPC164, CPC165, CPC167, CPC168, CPC169, CPC174, CPC176, CPC178
| CPC181, CPC182, CPC183, CPC184, CPC185, CPC187, CPC188, CPC189, CPC190
| CPC191, CPC192, CPC195, CPC196, CPC197, CPC207, CPC208, CPC212, CPC214
| CPC217, CPC220, CPC221, CPC222, CPC223, CPC224, CPC225, CPC231, CPC234
| CPC235, CPC301, CPC303, CPC304, CPC306, CPC307, CPC308, CPC309, CPC310
| CPC311, CPC312, CPC313, CPC314, CPC416, CPC417, CPC501, CPC503, CPC522
| CPC538, CPC540, CPC553, CPC561, CPC603, CPC604, CPC609, CPC611, CPC612
| CPC614, CPC618, CPC622, CPC702, CPC703, CPC704, CPC709, CPC711, CPC728
| CPC737, CPC739, CPC741, CPC742, CPC744, CPC745, CPC746, CPC758, CPC761
| CPC762, CPC801, CPC805, CPC806, CPC808, CPC809, CPC810, CBU3C1, CBU3C10
| CBU3C20, CU31C10, CU31C12, CU31C13, CU31C14, CU31C15, CU31C3, CU31C30, CU31C31
| CU31C4, CU31C5, CU31C6, CU31C7, CU31C8, CU31C9, CU31PC1, CU31PC11, CU31PC12
| CU31PC2, CU31PC21, CU31PC22, CU31PC23, CU31PC3, CU31PC4, CU31PU5C1, CU31PU5C2
| CU31U1C8, CU31U5C14, CU31U5C24, CU31U5C27, CU31U5C97, CU31U6C1, CU31U6C10
| CU31U6C12, CU31U6C14, CU31U6C2, CU31U6C3, CU31U6C5, CU31U6C7, CU31U6C8
| CU31U6C9, CU31X1, CU3CC170, CU3CC171, CU3CC190, CU3CPU1C3, CU3CPU2C3, CU3EC13
| CU3ECE1, CU3U1C1, CU3U1C12, CU3U1C129, CU3U1C132, CU3U1C20, CU3U1C21, CU3U1C24
| CU3U1C241, CU3U1C258, CU3U1C32, CU3U1C33, CU3U1C34, CU3U1C35, CU3U1C38
| CU3U1C4, CU3U1C41, CU3U1C44, CU3U1C47, CU3U1C52, CU3U1C55, CU3U1C58, CU3U1C62
| CAC1, CAC102, CAC13, CAC14, CAC15, CAC16, CAC2, CAC23, CAC28, CAC32, CAC48
| CAC49, CAC5, CAC6, CAU1C201, CAU1C209, CAU1C225, CAU1C227, CAU1C29, CEATXC12
| CEATXC15, CEATXC16, CEATXC20, CEATXC6, CEATXC8, CEMIC1, CEMIC10, CEMIC11
| CEMIC13, CEMIC15, CEMIC18, CEMIC2, CEMIC22, CEMIC27, CEMIC28, CEMIC29, CEMIC3
| CEMIC4, CEMIC5, CEMIC6, CEMIC7, CEMIC8, CEMIC9, CESDC10, CESDC12, CESDC13
| CESDC2, CESDC3, CESDC4, CESDC6, CESDC7, CESDO1C15, CESDO1C3, CESDO1C4, CESDO1C5
| CESDOC201, CESDOC203, CESDOC204, CESDOC405, CESDOC762, CESDU3CC1, CESDUC31
| CESDUC5, CESDUC6, CGC10, CGC11, CGC49, CGC5, CGC50, CGC51, CGC514, CGC515
| CGC516, CGC521, CGC522, CGC523, CGC524, CGC531, CGC532, CGC9, CGQ23C1, CGQX10C1
| CGQX11C1, CGQX12C1, CGQX13C1, CGU1C32, CGU1C4, CGU1C8, CHC10, CHC11, CHC12
| CHC13, CHC14, CHC16, CHC17, CHC18, CHC19, CHC20, CHC21, CHC22, CHC23, CHC25
| CHC26, CHC27, CHC28, CHC29, CHC3, CHC30, CHC9, CJC15, CK1C12, CK1C13, CK1C14
| CK1C5, CK1C6, CK1U1C111, CK1U1C122, CK1U1C131, CK1U1C14, CK1U1C23, CK1U1C42
| CK1U1C53, CK1U1C89, CKC1, CKC2, CKC21, CKC22, CKC3, CKC4, CKC5, CKCE1, CKCE2
| CO1C1, CO1C100, CO1C11, CO1C146, CO1C159, CO1C171, CO1C190, CO1C191, CO1C192
| CO1C2, CO1C30, COC207, COC208, COC210, COC217, COC251, COC252, COC300, COC303
| COC304, COC305, COC310, COC312, COC313, COC314, COC315, COC320, COC322
| COC323, COC324, COC325, COU1C224, COU1C231, COU1C245, COU1C253, COU1C424
| COU1C44, COU1C97, CPCE301, CPCE302, CPCE516, CPCE601, CSC1, CSC10, CSC11
| CSC114, CSC115, CSC13, CSC133, CSC134, CSC136, CSC139, CSC14, CSC140, CSC15
| CSC17, CSC174, CSC177, CSC178, CSC179, CSC18, CSC180, CSC181, CSC182, CSC183
| CSC184, CSC185, CSC186, CSC187, CSC188, CSC189, CSC191, CSC192, CSC193
| CSC194, CSC195, CSC196, CSC197, CSC198, CSC199, CSC2, CSC200, CSC201, CSC23
| CSC24, CSC25, CSC26, CSC31, CSC32, CSC35, CSC36, CSC4, CSC5, CSC521, CSC56
| CSC57, CSC6, CSC69, CSC7, CSC70, CSC71, CSC72, CSC73, CSC74, CSC75, CSC76
| CSC77, CSC78, CSC79, CSC80, CSC81, CSC82, CSC83, CSC84, CSC85, CSC86, CSC87
| CSC88, CSC89, CSC92, CSQ19C1, CSQ2C1, CSQ9C1, CSU31C1, CSU31C2, CTMC1, CTMC2
| CTMC3, CTMC4, CTQ1C1, CTQ2C1, CTQ2C2, CTQ2C3, CTQ5C1, CTX2, CUC730, CUC732
| CUC750, CUC751, CUC752, CUC756, CUC757, CUC759, CUCE1, CUCE2, CXQ1C1, CXQ1C2
Diode: | DOD202, DL1D1, DL1D2, DL1D98, D3D1, DU31D1, DU3CD51, DU3ED3, DU3ED51, DGD101
| DGD102, DGD103, DGD104, DGD12, DGD13, DO1D193, DSD3, DTD2, DTD3, DUD23, DUD24
| DUD7, DUD750, DUD8, DUD9
Transistor: | QU31PU2, QU31PU5, QU31Q1, QU31Q30, QU31Q31, QJQ7, QO1Q159, QO1Q190, QO1Q191
| QO1Q192, QOQ204, QPQ112, QPQ124, QPQ132, QPQ212, QPQ222, QPQ301, QPQ302
| QPQ303, QPQ305, QPQ307, QPQ411, QPQ513, QPQ713, QPQ714, QPQ770, QPQ771
| QPQ772, QPU601, QSQ3, QSQ35, QSQ36, QSQ40, QSQ45, QSQ47, QSQ48, QSQ49
| QSQ52, QSQ53, QSQ56, QSQ57, QSQ8, QTQ1, QTQ2, QTQ3, QTQ4, QTQ5, QUQ750
| QUQ751, QUQ756, QUQ757, QUQ759
2. No Test Nail |
Jumper: | RU3CR1, RU3CR2, RU3CR3, RU3CR4, RU3CR5, RU3CR6, RU3CR7, RU3CR8, RU3ER1, RU3ER2
| RU3ER3, RU3ER4, RU3ER91, RU3ER92, RU3ER93, RU3ER94, RU3ER95, RU3ER96, RU3ER97
| RU3ER98, JDVI, JHDMI, JHESINK1, JHESINK2, JUSB36
Resistor: | RGR1507
Capacitor: | CL1C3, CL1C4, CGCX10, CGCX11, CGCX12, CGCX13, CGCX14, CGCX15, CGCX16, CGCX27
| CGCX28, CGCX29, CGCX30, CGCX31, CGCX32, CGCX33, CGCX34, CGCX9, CGU1C41
| CGU1C42, CGU1C43, CGU1C44, CGU1C45, CGU1C46, CK1C3, CK1C4, CSC154, CSC155
| CSC156, CSC157, CSC158, CSC159, CSC160, CSC161, CSC162, CSC163, CSC164
| CSC165, CSK1C1, CSK1C2, CSL1C1, CSL1C2, CSX1, CTCX10, CTCX11, CTCX12, CTCX13
| CTCX14, CTCX15, CTCX18, CTCX19, CTCX2, CTCX21, CTCX22, CTCX23, CTCX24, CTCX25
| CTCX26, CTCX27, CTCX28, CTCX3, CTCX4, CTCX5, CTCX6, CTCX7, CTCX8, CTCX9
| CXCX1, CXCX10, CXCX11, CXCX12, CXCX13, CXCX14, CXCX15, CXCX16, CXCX17, CXCX18
| CXCX19, CXCX2, CXCX20, CXCX21, CXCX22, CXCX23, CXCX24, CXCX25, CXCX26, CXCX27
| CXCX28, CXCX29, CXCX3, CXCX30, CXCX31, CXCX32, CXCX4, CXCX5, CXCX6, CXCX7
| CXCX73, CXCX74, CXCX75, CXCX76, CXCX77, CXCX78, CXCX79, CXCX8, CXCX80, CXCX81
| CXCX82, CXCX9
3. Parallel |
Resistor: | RD3R2, RD3R4, RPR107, RPR119, RPR121, RPR127, RPR131, RPR136, RPR629
Capacitor: | CL1C11, CL1U1C11, CL1U1C222, CL1U1C232, CL1U1C24, CL1U1C3, CL1U1C30, CL1U1C8
| CL1X1, CD3C10, CD3C11, CD3C12, CD3C13, CD3C15, CD3C16, CD3C17, CD3C18, CD3C20
| CD3C21, CD3C23, CD3C24, CD3C25, CD3C26, CD3C27, CD3C28, CD3C29, CD3C3, CD3C30
| CD3C31, CD3C32, CD3C337, CD3C338, CD3C340, CD3C35, CD3C36, CD3C364, CD3C366
| CD3C4, CD3C5, CD3C53, CD3C54, CD3C6, CD3C7, CD3C74, CD3C8, CD3C9, CD3C91
| CD3C92, CD3C94, CD3C95, CF1C1, CPC112, CPC114, CPC117, CPC119, CPC125, CPC127
| CPC146, CPC147, CPC148, CPC152, CPC154, CPC156, CPC160, CPC161, CPC166
| CPC170, CPC171, CPC172, CPC173, CPC175, CPC177, CPC179, CPC180, CPC186
| CPC205, CPC206, CPC209, CPC211, CPC213, CPC215, CPC216, CPC218, CPC219
| CPC226, CPC227, CPC228, CPC229, CPC230, CPC302, CPC305, CPC533, CPC534
| CPC541, CPC544, CPC545, CPC546, CPC548, CPC550, CPC551, CPC601, CPC602
| CPC608, CPC610, CPC701, CPC726, CPC727, CPC729, CPC730, CPC734, CPC735
| CPC738, CPC747, CPC748, CPC749, CPC750, CPC753, CPC754, CPC755, CPC756
| CU31U5C1, CU31U5C12, CU31U5C19, CU31U5C25, CU31U6C4, CAGC1, CAGC2, CAGC3
| CAU1C1, CAU1C229, CAU1C25, CAU1C38, CAU1C9, CEMIC12, CEMIC14, CEMIC16, CEMIC17
| CEMIC19, CEMIC20, CEMIC21, CEMIC23, CEMIC24, CEMIC25, CEMIC26, CESDATC1
| CESDATC10, CESDATC4, CESDATC9, CESDU3EC1, CESDUC32, CESDUC4, CGC12, CGC13
| CGC14, CGC15, CGC517, CGC518, CGC519, CGU1C16, CGU1C17, CGU1C22, CGU1C23
| CGU1C30, CGU1C401, CHC24, CHC8, CK1PC2, CK1U1C103, CK1U1C3, CK1U1C32, CK1U1C47
| CK1U1C64, CK1U1C77, CK1U1C8, CK1U1C81, CK1U1C90, CK1U1C98, COC1, COU1C1
| COU1C10, COU1C24, COU1C51, COU1C57, COU310C2, COU320C2, CPCE101, CPCE102
| CPCE103, CPCE104, CPCE109, CPCE201, CPCE202, CPCE204, CPCE205, CPCE206
| CPCE515, CPCE517, CPCE706, CSC190, CSC205, CSC66, CSC68, CSC8, CSC9, CSX2
| CUCE5
ˇ¶TOP
Analog(MDA) Drive Through Component |
Resistor: | None.
Capacitor: | None.
ˇ¶TOP